<?xml version="1.0" encoding="UTF-8" ?>

<PropertyList>

	<name>Takeoff and climb</name>
	<description>This tutorial starts you at the end of runway 28R at San Francisco International Airport. You will learn how to take off and climb to 10,000 feet.</description>
	<timeofday type="string">noon</timeofday>
	<presets>
		<on-ground type="bool">true</on-ground>
		<latitude-deg>37.61415757</latitude-deg>
		<longitude-deg>-122.3570337</longitude-deg>
		<heading-deg>208.6</heading-deg>
		<airspeed-kt>0</airspeed-kt>
	</presets>

	<init>
		<set>
			<property>controls/flight/flaps</property>
			<value>0</value>
		</set>
		<set>
			<property>controls/gear/brake-parking</property>
			<value type="bool">true</value>
		</set>
		<set>
			<property>controls/lighting/nav-lights</property>
			<value type="bool">true</value>
		</set>
		<set>
			<property>controls/lighting/beacon</property>
			<value type="bool">true</value>
		</set>
		<set>
			<property>controls/lighting/logo-lights</property>
			<value type="bool">false</value>
		</set>
		<set>
			<property>controls/lighting/wing-lights</property>
			<value type="bool">false</value>
		</set>
		<set>
			<property>controls/lighting/taxi-lights</property>
			<value type="bool">true</value>
		</set>
		<set>
			<property>controls/lighting/landing-lights[0]</property>
			<value type="bool">false</value>
		</set>
		<set>
			<property>controls/lighting/landing-lights[1]</property>
			<value type="bool">false</value>
		</set>
		<set>
			<property>controls/lighting/landing-lights[2]</property>
			<value type="bool">false</value>
		</set>
		<set>
			<property>controls/engines/engine[0]/throttle</property>
			<value>0</value>
		</set>
		<set>
			<property>controls/engines/engine[0]/thrust-mode</property>
			<value>0</value>
		</set>
		<set>
			<property>controls/engines/engine[1]/throttle</property>
			<value>0</value>
		</set>
		<set>
			<property>controls/engines/engine[1]/thrust-mode</property>
			<value>0</value>
		</set>
		<set>
			<property>engines/engine[0]/running</property>
			<value type="bool">true</value>
		</set>
		<set>
			<property>engines/engine[1]/running</property>
			<value type="bool">true</value>
		</set>
		<nasal>
			<script><![CDATA[
			 CRJ700.instastart();
			]]></script>
		</nasal>
	</init>

	<step>
		<message>In this tutorial, we will learn how to take off and climb to 10,000 feet.</message>
	</step>

	<step>
		<message>First, deploy the flaps and slats to 8 degrees. Use [ and ] to extend/retract the flaps,
or use the control on the pedestal.</message>
		<view>
			<heading-offset-deg>337.2</heading-offset-deg>
			<pitch-offset-deg>-22.9</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.5</x-offset-m>
			<y-offset-m>-0.5</y-offset-m>
			<z-offset-m>-13.1</z-offset-m>
			<field-of-view>21.3</field-of-view>
		</view>
		<exit>
			<condition>
				<greater-than>
					<property>surface-positions/flap-pos-norm</property>
					<value>0.176</value>
				</greater-than>
			</condition>
		</exit>
	</step>

	<step>
		<message>Before we take off, turn on all 3 landing lights and turn off the taxi light.</message>
		<view>
			<heading-offset-deg>327.4</heading-offset-deg>
			<pitch-offset-deg>13.2</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.5</x-offset-m>
			<y-offset-m>-0.5</y-offset-m>
			<z-offset-m>-13.1</z-offset-m>
			<field-of-view>27.6</field-of-view>
		</view>
		<marker>
			<x-m>-13.7000</x-m>
			<y-m>-0.1317</y-m>
			<z-m>-0.3075</z-m>
			<scale>4.8167</scale>
		</marker>
		<exit>
			<condition>
				<and>
					<property>controls/lighting/landing-lights[0]</property>
					<property>controls/lighting/landing-lights[1]</property>
					<property>controls/lighting/landing-lights[2]</property>
					<not>
						<property>controls/lighting/taxi-lights</property>
					</not>
				</and>
			</condition>
		</exit>
	</step>
	<step>
		<message>This is the throttle quadrant. Right now, the thrust computers for each engine
are in "manual" mode, which means you control the engines with your throttle. For takeoff, we will be
switching them to "TO/GA" mode, which means "takeoff/go around power." This gives us additional power
during this critical stage of flight.</message>
		<view>
			<heading-offset-deg>316.4</heading-offset-deg>
			<pitch-offset-deg>-43.1</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.5</x-offset-m>
			<y-offset-m>-0.5</y-offset-m>
			<z-offset-m>-13.1</z-offset-m>
			<field-of-view>17.1</field-of-view>
		</view>
	</step>
	<step>
		<message>Thrust modes for each engine can be cycled by middle-clicking the respective
thrust lever, or you can use the shortcut key Ctrl-T to cycle both at the same time.</message>
	</step>

	<step>
		<message>Assuming there's nobody already there, taxi onto the runway. Don't forget to
use the tiller, if enabled. When you're lined up, press Ctrl-T twice to move the thrust
levers into "TO/GA" mode. This will initiate your takeoff.</message>
		<view>
			<heading-offset-deg>0.0</heading-offset-deg>
			<pitch-offset-deg>0.0</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.5</x-offset-m>
			<y-offset-m>-0.5</y-offset-m>
			<z-offset-m>-13.1</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>
		<exit>
			<condition>
				<and>
					<not>
						<property>controls/gear/brake-parking</property>
					</not>
					<equals>
						<property>controls/engines/engine[0]/thrust-mode</property>
						<value>2</value>
					</equals>
					<equals>
						<property>controls/engines/engine[1]/thrust-mode</property>
						<value>2</value>
					</equals>
				</and>
			</condition>
		</exit>
	</step>

	<step>
		<message>Proceed down the runway. Rotate the nose into the air at approximately 150 knots.
When you get into the air, press Ctrl-T twice again to move the thrust levers back to the manual position.</message>
		<exit>
			<condition>
				<and>
					<not>
						<property>gear/gear[0]/wow</property>
					</not>
					<not>
						<property>gear/gear[1]/wow</property>
					</not>
					<not>
						<property>gear/gear[2]/wow</property>
					</not>
					<equals>
						<property>controls/engines/engine[0]/thrust-mode</property>
						<value>0</value>
					</equals>
					<equals>
						<property>controls/engines/engine[1]/thrust-mode</property>
						<value>0</value>
					</equals>
				</and>
			</condition>
		</exit>
	</step>

	<step>
		<message>We're in the air! Retract the flaps and slats and raise the gear.</message>
		<exit>
			<condition>
				<and>
					<not>
						<property>controls/gear/gear-down</property>
					</not>
					<equals>
						<property>controls/flight/flaps</property>
						<value>0</value>
					</equals>
				</and>
			</condition>
		</exit>
	</step>

	<step>
		<message>Maintain a steady 2,000-FPM climb and continue towards 10,000 feet. Remember
to stay below 250 KIAS until you reach 10,000 feet.</message>
		<exit>
			<condition>
				<greater-than>
					<property>instrumentation/altimeter[0]/indicated-altitude-ft</property>
					<value>10000</value>
				</greater-than>
			</condition>
		</exit>
	</step>

	<end>
		<message>Okay, you've made a successful takeoff and climb. Enjoy the rest of your flight!
HINT: You can set the thrust levers to "climb" mode to maintain a 300-knot climb at 90% N1.</message>
	</end>

</PropertyList>
