// Copyright (C) 2017 The Qt Company Ltd.
// SPDX-License-Identifier: LicenseRef-Qt-Commercial OR GFDL-1.3-no-invariants-only

/*!
    \example heartrate-game
    \title Bluetooth Low Energy Heart Rate Game
    \examplecategory {Connectivity}
    \brief A game demonstrating the interaction with a Bluetooth Low Energy Heart Rate
    device/service.

    The Bluetooth Low Energy Heart Rate Game shows how to develop a Bluetooth Low Energy
    application using the Qt Bluetooth API. The application covers the scanning for
    Bluetooth Low Energy devices, connecting to a Heart Rate service on the device, writing
    characteristics and descriptors, and receiving updates from the device once the heart rate
    has changed.

    \image heartgame-start.png

    The example introduces the following Qt classes:

    \list
        \li \l QLowEnergyController
        \li \l QLowEnergyService
        \li \l QLowEnergyCharacteristic
        \li \l QLowEnergyDescriptor
    \endlist

    A Bluetooth Low Energy device with a Heart Rate
    service is required for this application to work. An alternative might be a programmable
    Bluetooth Low Energy device which might simulate the service. You can also use the
    \l {heartrate-server} {Heart Rate server} example for that purpose.
    If no such device is available, a demo mode is available which creates and displays
    random values. This demo mode is enabled by passing \c{--simulator} on the
    command line.

    The goal of the game is to increase the measured heart rate as much as possible.

    A detailed explanation of the APIs used in this example is given in the
    \l {Using Qt Bluetooth Low Energy API} section of the Qt Bluetooth module
    documentation.

    The \l {lowenergyscanner}{Bluetooth Low Energy Scanner} example might be more suitable
    if a heart rate device is not available. The scanner example works with any type of Bluetooth
    Low Energy peripheral device.

    \include examples-run.qdocinc

    \section1 Visual Tour

    The application searches for all Bluetooth Low Energy peripheral devices in the vicinity.
    It is assumed that the remote devices advertise their presence. The found devices are
    presented in a list. Note that all found Bluetooth Low Energy devices are listed even
    if they do not offer a Heart Rate service.

    \image heartgame-search.png

    After the user has selected a target device, the example connects to its Heart Rate service
    if one is available. It automatically enables notification updates for the Heart Rate value
    and presents the current value on the screen.

    \image heartgame-running.png

    Once the monitoring process is canceled, a small graph presents a summary of the received
    values.

    \image heartgame-result.png

*/
