/** \file
 *
 *  This file contains special DoxyGen information for the generation of the main page and other special
 *  documentation pages. It is not a project source file.
 */
 
/** \mainpage Audio Output Device Demo
 *  
 *  Audio demonstration application. This gives a simple reference
 *  application for implementing a USB Audio Output device using the
 *  basic USB Audio drivers in all modern OSes (i.e. no special drivers
 *  required).
 *  
 *  On startup the system will automatically enumerate and function
 *  as a USB speaker. Incomming audio will output in 8-bit PWM onto
 *  the timer output (timer 3 for the AT90USBXXX6/7 USB AVRs, timer 1 for
 *  the AT90USBXXX2 controller AVRs) compare channel A for AUDIO_OUT_MONO
 *  mode, on channels A and B for AUDIO_OUT_STEREO and on the board LEDs
 *  for AUDIO_OUT_LEDS mode. Decouple audio outputs with a capacitor and
 *  attach to a speaker to hear the audio.
 *  
 *  Under Windows, if a driver request dialogue pops up, select the option
 *  to automatically install the appropriate drivers.
 *  
 *
 *  <table>
 *   <tr>
 *    <td><b>USB Mode:</b></td>
 *    <td>Device</td>
 *   </tr>
 *   <tr>
 *    <td><b>USB Class:</b></td>
 *    <td>Audio Class</td>
 *   </tr>
 *   <tr> 
 *    <td><b>USB Subclass:</b></td>
 *    <td>Standard Audio Device</td>
 *   </tr>
 *   <tr>
 *    <td><b>Relevant Standards:</b></td>
 *    <td>USBIF Audio Class Specification</td>
 *    <td>USBIF Audio Class Terminal Types Specification</td>
 *    <td>USBIF Audio Data Formats Specification</td>
 *   </tr>
 *   <tr>
 *    <td><b>Usable Speeds:</b></td>
 *    <td>Full Speed Mode</td>
 *   </tr>
 *  </table>
 */