No.     Time           Source                Destination           Protocol Length Info       src port dst port Leftover Capture Data
    246 14.396810      localhost ()          Shenzhen_05:5b:59 (Electronic Scale) RFCOMM   13                                  

Frame 246: 13 bytes on wire (104 bits), 13 bytes captured (104 bits)
Bluetooth
Bluetooth HCI H4
Bluetooth HCI ACL Packet
Bluetooth L2CAP Protocol
Bluetooth RFCOMM Protocol
    Address: E/A flag: 1, C/R flag: 1, Direction: 0, Channel: 0
    Control: Frame type: Set Asynchronous Balanced Mode (SABM) (0x2f), P/F flag: 1
    Payload length: 0
    Frame Check Sequence: 0x1c

No.     Time           Source                Destination           Protocol Length Info       src port dst port Leftover Capture Data
    248 14.402371      Shenzhen_05:5b:59 (Electronic Scale) localhost ()          RFCOMM   13                                  

Frame 248: 13 bytes on wire (104 bits), 13 bytes captured (104 bits)
Bluetooth
Bluetooth HCI H4
Bluetooth HCI ACL Packet
Bluetooth L2CAP Protocol
Bluetooth RFCOMM Protocol
    Address: E/A flag: 1, C/R flag: 1, Direction: 0, Channel: 0
    Control: Frame type: Unnumbered Acknowledgement (UA) (0x63), P/F flag: 1
    Payload length: 0
    Frame Check Sequence: 0xd7

No.     Time           Source                Destination           Protocol Length Info       src port dst port Leftover Capture Data
    249 14.403103      localhost ()          Shenzhen_05:5b:59 (Electronic Scale) RFCOMM   23                                  

Frame 249: 23 bytes on wire (184 bits), 23 bytes captured (184 bits)
Bluetooth
Bluetooth HCI H4
Bluetooth HCI ACL Packet
Bluetooth L2CAP Protocol
Bluetooth RFCOMM Protocol
    Address: E/A flag: 1, C/R flag: 1, Direction: 0, Channel: 0
    Control: Frame type: Unnumbered Information with Header check (UIH) (0xef), P/F flag: 0
    Payload length: 10
    Multiplexer Control Command
        Type: DLC Parameter Negotiation (PN) (0x20), C/R flag = 1, E/A flag = 1
        MCC Length: 8
        00.. .... = Zeros padding: 0x0
        ..00 1100 = MCC DLCI: 0x0c (Direction: 0, Channel: 6)
        I1-I4: 0x0, C1-C4: 0xf
        ..00 0000 = Priority: 0
        Acknowledgement Timer T1: 0(0 ms)
        Max Frame Size: 990
        Maximum number of retransmissions: 0
        .... .111 = Error Recovery Mode: 7
    Frame Check Sequence: 0x70

No.     Time           Source                Destination           Protocol Length Info       src port dst port Leftover Capture Data
    251 14.409794      Shenzhen_05:5b:59 (Electronic Scale) localhost ()          RFCOMM   7                                   

Frame 251: 7 bytes on wire (56 bits), 7 bytes captured (56 bits)
Bluetooth
Bluetooth HCI H4
Bluetooth HCI ACL Packet
Bluetooth L2CAP Protocol
Bluetooth RFCOMM Protocol
    Address: E/A flag: 1, C/R flag: 0, Direction: 0, Channel: 0
    Control: Frame type: Unnumbered Information with Header check (UIH) (0xef), P/F flag: 0
    Payload length: 10
    Multiplexer Control Command
        Type: DLC Parameter Negotiation (PN) (0x20), C/R flag = 0, E/A flag = 1
        MCC Length: 8
        00.. .... = Zeros padding: 0x0
        ..00 1100 = MCC DLCI: 0x0c (Direction: 0, Channel: 6)
        I1-I4: 0x0, C1-C4: 0xe
        ..00 0111 = Priority: 7
        Acknowledgement Timer T1: 0(0 ms)
        Max Frame Size: 990
        Maximum number of retransmissions: 0
        .... .010 = Error Recovery Mode: 2
    Frame Check Sequence: 0xaa

No.     Time           Source                Destination           Protocol Length Info       src port dst port Leftover Capture Data
    261 14.552701      localhost ()          Shenzhen_05:5b:59 (Electronic Scale) RFCOMM   13                                  

Frame 261: 13 bytes on wire (104 bits), 13 bytes captured (104 bits)
Bluetooth
Bluetooth HCI H4
Bluetooth HCI ACL Packet
Bluetooth L2CAP Protocol
Bluetooth RFCOMM Protocol
    Address: E/A flag: 1, C/R flag: 1, Direction: 0, Channel: 6
    Control: Frame type: Set Asynchronous Balanced Mode (SABM) (0x2f), P/F flag: 1
    Payload length: 0
    Frame Check Sequence: 0x43

No.     Time           Source                Destination           Protocol Length Info       src port dst port Leftover Capture Data
    263 14.559806      Shenzhen_05:5b:59 (Electronic Scale) localhost ()          RFCOMM   13                                  

Frame 263: 13 bytes on wire (104 bits), 13 bytes captured (104 bits)
Bluetooth
Bluetooth HCI H4
Bluetooth HCI ACL Packet
Bluetooth L2CAP Protocol
Bluetooth RFCOMM Protocol
    Address: E/A flag: 1, C/R flag: 1, Direction: 0, Channel: 6
    Control: Frame type: Unnumbered Acknowledgement (UA) (0x63), P/F flag: 1
    Payload length: 0
    Frame Check Sequence: 0x88

No.     Time           Source                Destination           Protocol Length Info       src port dst port Leftover Capture Data
    264 14.560556      localhost ()          Shenzhen_05:5b:59 (Electronic Scale) RFCOMM   17                                  

Frame 264: 17 bytes on wire (136 bits), 17 bytes captured (136 bits)
Bluetooth
Bluetooth HCI H4
Bluetooth HCI ACL Packet
Bluetooth L2CAP Protocol
Bluetooth RFCOMM Protocol
    Address: E/A flag: 1, C/R flag: 1, Direction: 0, Channel: 0
    Control: Frame type: Unnumbered Information with Header check (UIH) (0xef), P/F flag: 0
    Payload length: 4
    Multiplexer Control Command
        Type: Modem Status Command (MSC) (0x38), C/R flag = 1, E/A flag = 1
        MCC Length: 2
        0011 00.. = MCC DLCI: 0x0c (Direction: 0, Channel: 6)
        .... ..1. = Ones padding: 0x1
        .... ...1 = EA Flag: Last field octet (0x1)
        V.24 Signals: FC = 0, RTC = 1, RTR = 1, IC = 0, DV = 1
    Frame Check Sequence: 0x70

No.     Time           Source                Destination           Protocol Length Info       src port dst port Leftover Capture Data
    265 14.561669      Shenzhen_05:5b:59 (Electronic Scale) localhost ()          RFCOMM   18                                  

Frame 265: 18 bytes on wire (144 bits), 18 bytes captured (144 bits)
Bluetooth
Bluetooth HCI H4
Bluetooth HCI ACL Packet
Bluetooth L2CAP Protocol
Bluetooth RFCOMM Protocol
    Address: E/A flag: 1, C/R flag: 0, Direction: 0, Channel: 0
    Control: Frame type: Unnumbered Information with Header check (UIH) (0xef), P/F flag: 0
    Payload length: 4
    Multiplexer Control Command
        Type: Modem Status Command (MSC) (0x38), C/R flag = 1, E/A flag = 1
        MCC Length: 2
        0011 00.. = MCC DLCI: 0x0c (Direction: 0, Channel: 6)
        .... ..1. = Ones padding: 0x1
        .... ...1 = EA Flag: Last field octet (0x1)
        V.24 Signals: FC = 0, RTC = 1, RTR = 1, IC = 0, DV = 1
    Frame Check Sequence: 0xaa

No.     Time           Source                Destination           Protocol Length Info       src port dst port Leftover Capture Data
    266 14.562437      localhost ()          Shenzhen_05:5b:59 (Electronic Scale) RFCOMM   17                                  

Frame 266: 17 bytes on wire (136 bits), 17 bytes captured (136 bits)
Bluetooth
Bluetooth HCI H4
Bluetooth HCI ACL Packet
Bluetooth L2CAP Protocol
Bluetooth RFCOMM Protocol
    Address: E/A flag: 1, C/R flag: 1, Direction: 0, Channel: 0
    Control: Frame type: Unnumbered Information with Header check (UIH) (0xef), P/F flag: 0
    Payload length: 4
    Multiplexer Control Command
        Type: Modem Status Command (MSC) (0x38), C/R flag = 0, E/A flag = 1
        MCC Length: 2
        0011 00.. = MCC DLCI: 0x0c (Direction: 0, Channel: 6)
        .... ..1. = Ones padding: 0x1
        .... ...1 = EA Flag: Last field octet (0x1)
        V.24 Signals: FC = 0, RTC = 1, RTR = 1, IC = 0, DV = 1
    Frame Check Sequence: 0x70

No.     Time           Source                Destination           Protocol Length Info       src port dst port Leftover Capture Data
    268 14.568450      Shenzhen_05:5b:59 (Electronic Scale) localhost ()          RFCOMM   18                                  

Frame 268: 18 bytes on wire (144 bits), 18 bytes captured (144 bits)
Bluetooth
Bluetooth HCI H4
Bluetooth HCI ACL Packet
Bluetooth L2CAP Protocol
Bluetooth RFCOMM Protocol
    Address: E/A flag: 1, C/R flag: 0, Direction: 0, Channel: 0
    Control: Frame type: Unnumbered Information with Header check (UIH) (0xef), P/F flag: 0
    Payload length: 4
    Multiplexer Control Command
        Type: Modem Status Command (MSC) (0x38), C/R flag = 0, E/A flag = 1
        MCC Length: 2
        0011 00.. = MCC DLCI: 0x0c (Direction: 0, Channel: 6)
        .... ..1. = Ones padding: 0x1
        .... ...1 = EA Flag: Last field octet (0x1)
        V.24 Signals: FC = 0, RTC = 1, RTR = 1, IC = 0, DV = 1
    Frame Check Sequence: 0xaa

No.     Time           Source                Destination           Protocol Length Info       src port dst port Leftover Capture Data
    270 14.789246      localhost ()          Shenzhen_05:5b:59 (Electronic Scale) SPP      22                                  

Frame 270: 22 bytes on wire (176 bits), 22 bytes captured (176 bits)
Bluetooth
Bluetooth HCI H4
Bluetooth HCI ACL Packet
Bluetooth L2CAP Protocol
Bluetooth RFCOMM Protocol
    Address: E/A flag: 1, C/R flag: 1, Direction: 0, Channel: 6
    Control: Frame type: Unnumbered Information with Header check (UIH) (0xef), P/F flag: 1
    Payload length: 8
    Credits: 3
    Frame Check Sequence: 0x53
Bluetooth SPP Packet
    Data: fe020100b935018e

No.     Time           Source                Destination           Protocol Length Info       src port dst port Leftover Capture Data
    274 14.825308      Shenzhen_05:5b:59 (Electronic Scale) localhost ()          RFCOMM   15                                  

Frame 274: 15 bytes on wire (120 bits), 15 bytes captured (120 bits)
Bluetooth
Bluetooth HCI H4
Bluetooth HCI ACL Packet
Bluetooth L2CAP Protocol
Bluetooth RFCOMM Protocol
    Address: E/A flag: 1, C/R flag: 0, Direction: 0, Channel: 6
    Control: Frame type: Unnumbered Information with Header check (UIH) (0xef), P/F flag: 1
    Payload length: 0
    Credits: 1
    Frame Check Sequence: 0x89

No.     Time           Source                Destination           Protocol Length Info       src port dst port Leftover Capture Data
    338 22.421742      Shenzhen_05:5b:59 (Electronic Scale) localhost ()          SPP      31                                  

Frame 338: 31 bytes on wire (248 bits), 31 bytes captured (248 bits)
Bluetooth
Bluetooth HCI H4
Bluetooth HCI ACL Packet
Bluetooth L2CAP Protocol
Bluetooth RFCOMM Protocol
    Address: E/A flag: 1, C/R flag: 0, Direction: 0, Channel: 6
    Control: Frame type: Unnumbered Information with Header check (UIH) (0xef), P/F flag: 1
    Payload length: 16
    Credits: 0
    Frame Check Sequence: 0x89
Bluetooth SPP Packet
    Data: cf02b5b9037100e81d025e0d023206f7

No.     Time           Source                Destination           Protocol Length Info       src port dst port Leftover Capture Data
    339 22.449212      Shenzhen_05:5b:59 (Electronic Scale) localhost ()          SPP      31                                  

Frame 339: 31 bytes on wire (248 bits), 31 bytes captured (248 bits)
Bluetooth
Bluetooth HCI H4
Bluetooth HCI ACL Packet
Bluetooth L2CAP Protocol
Bluetooth RFCOMM Protocol
    Address: E/A flag: 1, C/R flag: 0, Direction: 0, Channel: 6
    Control: Frame type: Unnumbered Information with Header check (UIH) (0xef), P/F flag: 1
    Payload length: 16
    Credits: 0
    Frame Check Sequence: 0x89
Bluetooth SPP Packet
    Data: cf02b5b9037100e81d025e0d023206f7
